DOOR LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

id091400817300

1. Position the door glass so that the distance between the top of the front door glass and top of the front beltline molding is 110 mm {4.33 in}.

e5u912zw5002

2. Disconnect the negative battery cable.(See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Door trim (See DOOR TRIM REMOVAL/INSTALLATION.)

  (2) Door speaker (See DOOR SPEAKER REMOVAL/INSTALLATION.)

  (3) Inner handle (See INNER HANDLE REMOVAL/INSTALLATION.)

  (4) Door module panel (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

  (5) Door glass (See DOOR GLASS REMOVAL/INSTALLATION.)

4. Detach the rods from the key cylinder and the outer handle.

5. Remove the screws, then remove the door latch and lock actuator.

e5u914aw4006

6. Install in the reverse order of removal.