DOOR ADJUSTMENT

id091100521100

1. Measure the gap and height difference between the door and the body.

2. Loosen the door hinge installation bolts or the door lock striker installation screws, and adjust the door.

3. Tighten the bolts or screws.

amxzzw00000165

  Standard clearance

  A—A top and bottom (a): 3.1—5.0 mm {0.13—0.19 in}
  A—A middle (a): 3.3—5.2 mm {0.13—0.20 in}
  B—B top (b): -1.0—1.0 mm {-0.040—0.039 in}
  B—B bottom (b): -0.5—1.5 mm {-0.020—0.059 in}
  C—C top and bottom (c): 3.0—5.0 mm {0.12—0.19 in}
  C—C top (c): -1.0—1.0 mm {-0.040—0.039 in}
  C—C bottom (d): -0.5—1.5 mm {-0.020—0.059 in}