POWER RETRACTABLE HARDTOP CONTROL MODULE REMOVAL/INSTALLATION

id091600821700

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF])

3. Remove the service hole cover (LH) of the back trim.

4. Partially peel back the power retractable hardtop cover.

5. Remove the roof hook cable case.

amxzzw00000910

6. Remove in the order indicated in the table.

amxzzw00000911

1 | Nut
2 | Connector
3 | Power retractable hardtop control module

7. Install in the reverse order of removal.