FRONT FOG LIGHT BULB REMOVAL/INSTALLATION

id091800468600

Vehicles With Active Bonnet

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the fasteners.

amxzzw00002700

4. Slightly bend back the mudguard.

5. Disconnect the front fog light connector.

amxzzw00002701

6. Rotate the front fog light bulb in the direction of the arrow shown in the figure and remove it.

amxzzw00002702

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When handling the bulb, hold the flange, not the glass. Wipe off any finger prints before installation.

7. Install in the reverse order of removal.

Vehicles Without Active Bonnet

Type A

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the fasteners.

amxzzw00002700

4. Slightly bend back the mudguard.

5. Disconnect the front fog light connector.

amxzzw00002709

6. Rotate the front fog light bulb in the direction of the arrow shown in the figure and remove it.

amxzzw00002710

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When handling the bulb, hold the flange, not the glass. Wipe off any finger prints before installation.

7. Install in the reverse order of removal.

Type B

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the fasteners, then slightly bend back the mudguard.

4. Disconnect the front fog light connector.

amxzzw00001048

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When handling the bulb, hold the flange, not the glass.

5. Remove the front fog light bulb.

6. Install in the reverse order of removal.