TFT CHECK CONNECTOR OUTLINE [SJ6A-EL]

id051311640200

• When the following operation is performed, the AT warning light illuminates according to the ATF temperature.

  1. Short the TFT check connector terminal A and B of the TCM.

  ar8wzw00000248

  2. Continue the shifting operation from N to D, D to N within 1.5 s until the AT warning light illuminates.

AT warning light illumination chart for ATF level adjustment

ATF condition | Time chart
--- | ---
ATF Temperature below 50 °C {122 °F} • ATF temperature is lower than a ATF level adjustable temperature. |
ATF Temperature 50—60 °C {122—140 °F} • ATF temperature is same a ATF level adjustable temperature. |
ATF Temperature above 60 °C {140 °F} • ATF temperature is higher than a ATF level adjustable temperature. |