PLASTIC PARTS HEAT RESISTING TEMPERATURE [PLASTIC BODY PARTS]

id098011740200

Part Name | Code | Material Name | Heat resisting Temperature°C{°F}
--- | --- | --- | ---
FRONT COMBINATION LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 125 {257}
FRONT BUMPER | PP | POLYPROPYLENE | 110 {230}
FRONT SIDE MARKER LIGHT | LENS | AS | AS | 95 {203}
HOUSING | ABS | ABS | 88 {190}
POWER OUTER MIRROR | BASE | ABS | ABS | 85 {185}
BODY | ABS | ABS | 85 {185}
VISOR | AAS | AAS | 88 {190}
SIDE STEP MOLDING | PP | POLYPROPYLENE | 110 {230}
REAR BUMPER | PP | POLYPROPYLENE | 110 {230}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 95 {203}
HOUSING | AES | AES | 90 {194}
OUTER HANDLE | LEVER | PC-PBT | POLYCARBONATE-PBT | 80 {176}
BASE | PC-PET | POLYCARBONATE-PET | 80 {176}
HIGH-MOUNT BRAKE LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PC | POLYCARBONATE | 130 {266}
REFLECTOR | LENS | PMMA | ACRYLIC | 90 {194}
HOUSING | ABS | ABS | 88 {190}
REAR DECK PLATE | ABS | ABS | 100 {212}

  Note
  • The application of temperatures higher than heat resisting temperatures may result in part deformation.