AIR CLEANER ELEMENT INSPECTION [L8, LF]

id0113a3800800

1. Remove the air cleaner element. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

2. Inspect the following items:

  • Has the replacement interval come?
  • Is the air cleaner element soiled, damaged, or bent?
  • Are the air cleaner case and the air cleaner element correctly sealed?
  • Is the correct air cleaner element installed?
    ― If there is any abnormality, clean or replace the air cleaner element. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)