INTERLOCK CABLE INSPECTION

id051400254300

1. Turn the ignition switch to the ON position. (engine off)

2. Remove the clip of the selector lever base plate, then remove the interlock cable from the U-groove.

L.H.D.

amxzzw00000231

R.H.D.

amxzzw00000232

3. Remove the interlock cable from the selector lever.

L.H.D.

amxzzw00000233

R.H.D.

amxzzw00000234

4. Verify that the interlock cable moves freely with the brake pedal depressed.

amxzzw00000235

  • If there is any malfunction, replace the interlock cable.