BASIC INSPECTION [SJ6A-EL]

id050307800300

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Measure the battery voltage. • Is the battery voltage 10.0—14.0 V? | Yes | Go to the next step.
No | Replace or recharge the battery. (See BATTERY REMOVAL/INSTALLATION [L8, LF].) (See BATTERY RECHARGING [L8, LF].)
2 | • Inspect the TCM related harnesses, connectors and fuses. • Is there any malfunction? | Yes | Repair or replace any malfunctioning part according to the inspection results.
No | Go to the next step.
3 | • Warm up the engine to normal operating temperature. • Retrieve DTC using the M-MDS. (See AUTOMATIC TRANSMISSION ON-BOARD DIAGNOSTIC FUNCTION [SJ6A-EL].) • Are any DTCs present? | Yes | Record the Freeze Frame Data and perform the appropriate DTC troubleshooting procedures. (See DTC TABLE [SJ6A-EL].)
No | Go to the next step.
4 | • Inspect the ATF color and condition. (See AUTOMATIC TRANSMISSION FLUID (ATF) INSPECTION [SJ6A-EL].) • Are ATF color and odor normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning part according to the inspection results. Flush AT and cooler line if necessary.
5 | • Perform the road test. (See ROAD TEST [SJ6A-EL].) • Is the AT operating normally? | Yes | Go to the next step.
No | Repair or replace any malfunctioning part according to the inspection results.
6 | • Perform the time lag test. (See MECHANICAL SYSTEM TEST [SJ6A-EL].) • Is the AT operating normally? | Yes | Go to the next step.
No | Repair or replace any malfunctioning part according to the inspection results.
7 | • Perform the stall test. (See MECHANICAL SYSTEM TEST [SJ6A-EL].) • Is the stall speed within the specified? | Yes | Go to the next step.
No | Repair or replace any malfunctioning part according to the inspection results.
8 | • Perform the line pressure test. (See MECHANICAL SYSTEM TEST [SJ6A-EL].) • Is the line pressure within the specified? | Yes | Go to the next step.
No | Repair or replace any malfunctioning part according to the inspection results.
9 | • Inspect the following part or signal related PIDs using the M-MDS: (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) (See PID/DATA MONITOR INSPECTION [SJ6A-EL].) PCM PIDs: ― APP ― TP REL ― VSS ― BOO ― RPM ― ECT TCM PIDs: ― THOP ― TSS ― OSS ― TFT ― TR ― MNL SW ― UP SW ― DWN SW ― BOO TCM • Are they normal? (See PCM INSPECTION [L8, LF].) (See PID/DATA MONITOR INSPECTION [SJ6A-EL].) | Yes | Perform the symptom troubleshooting and follow the procedures.
No | Repair or replace any malfunctioning part according to the inspection results.