CONTROL VALVE BODY DISASSEMBLY/ASSEMBLY

id051300261800

Components

bsj6za00000896

1 | Shift solenoid C
2 | Shift solenoid B
3 | Shift solenoid D
4 | Shift solenoid A
5 | Shift solenoid E
6 | Shift solenoid F
7 | Pressure control solenoid
8 | Shift solenoid G
9 | TCC control solenoid
10 | Harness clip

Disassembly Procedure

  Caution
  • Do not damage the solenoid.

1. Remove the shift solenoid C from the control valve body.

bsj6za00000221

  Caution
  • Do not damage the solenoid.

2. Remove the shift solenoid B shift solenoid D from the control valve body.

bsj6za00000222

3. Remove the bolt and the wiring harness clip.

  Caution
  • Do not damage the solenoid.

4. Remove the shift solenoid A from the control valve body.

bsj6za00000223

  Caution
  • Do not damage the solenoid.

5. Remove the shift solenoid E from the control valve body.

bsj6za00000224

Assembly Procedure

  Caution
  • Do not damage the solenoid.

1. Install the shift solenoid E to the control valve body.

bsj6za00000224

  Tightening torque

  8.0—12.0 N·m {81.6—122.3 kgf·cm, 70.9—106.1 in·lbf}

2. Install the bolt and the wiring harness clip.

  Caution
  • Do not damage the solenoid.

3. Install the shift solenoid A to the control valve body.

bsj6za00000223

  Tightening torque

  8.0—12.0 N·m {81.6—122.3 kgf·cm, 70.9—106.1 in·lbf}

  Caution
  • Do not damage the solenoid.

4. Install the shift solenoid B and the shift solenoid D to the control valve body.

bsj6za00000222

  Tightening torque

  8.0—12.0 N·m {81.6—122.3 kgf·cm, 70.9—106.1 in·lbf}

  Caution
  • Do not damage the solenoid.

5. Install the shift solenoid C to the control valve body.

bsj6za00000221

  Tightening torque

  8.0—12.0 N·m {81.6—122.3 kgf·cm, 70.9—106.1 in·lbf}