DLC-2 CONSTRUCTION [ABS]

id0402a7100600

• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.
• Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this connector. The connector has a 16-pin construction that includes the CAN_H (HS), CAN_L (HS), GND1, GND2 and B+ terminals.

amxzzn00000122

Terminal | Function
--- | ---
CAN_L (HS) | Serial communication Lo terminal (HS)
CAN_H (HS) | Serial communication Hi terminal (HS)
GND1 | Body ground terminal
GND2 | Serial communication ground terminal
B+ | Battery power supply terminal