DTC B00D2:29 [ACTIVE BONNET]

id0802f1826700

DESCRIPTION | Active bonnet warning light communication error
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the diagnostic procedure. • Warning light illumination request output from active bonnet control module and warning light control report input from instrument cluster are incompatible
POSSIBLE CAUSE | • Improper assembly of instrument cluster • Instrument cluster malfunction • Active bonnet control module malfunction

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | VERIFY IF OTHER DTCs ARE DISPLAYED • Clear the DTC for the active bonnet control module using the M-MDS. (See CLEARING DTC [ACTIVE BONNET].) • Perform the active bonnet control module DTC inspection using the M-MDS. (See DTC INSPECTION [ACTIVE BONNET].) • Is DTC U0001:88 or U0155:00 displayed? | Yes | Perform the applicable DTC troubleshooting. (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
No | Go to the next step.
2 | INSPECT INSTRUMENT CLUSTER • Verify that the instrument cluster is correctly installed. • Is the instrument cluster correctly installed? | Yes | Go to the next step.
No | Install the instrument cluster correctly. (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.) Go to the next step.
3 | INSPECT INSTRUMENT CLUSTER • Verify the warning light illumination using the instrument cluster input/output check mode. (See INSTRUMENT CLUSTER INPUT/OUTPUT CHECK MODE.) ― Check code 26 • Does the active bonnet warning illuminate? | Yes | Go to the next step.
No | Replace the instrument cluster. (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.) Go to the next step.
4 | PERFORM DTC INSPECTION FOR ACTIVE BONNET CONTROL MODULE • Clear the DTC for the active bonnet control module using the M-MDS. (See CLEARING DTC [ACTIVE BONNET].) • Perform the active bonnet control module DTC inspection using the M-MDS. (See DTC INSPECTION [ACTIVE BONNET].) • Is the same DTC displayed? | Yes | Replace the active bonnet control module. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.