REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION [MANUAL AIR CONDITIONER]

id0740a2802600

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Discharge the refrigerant from the system. (See REFRIGERANT CHARGING.)

4. Remove in the order indicated in the table.

e5u740zw5026

1 | Refrigerant pressure switch connector
2 | Refrigerant pressure switch (See Refrigerant Pressure Switch Installation Note.)

5. Install in the reverse order of removal.

Refrigerant Pressure Switch Installation Note

1. Apply compressor oil to the O-ring joints.