NO. 10 OIL PRESSURE GAUGE INDICATION IS DEFECTIVE (OIL PRESSURE GAUGE NEEDLE DOES NOT MOVE FROM THE L POSITION OR LESS) [INSTRUMENT CLUSTER]

id0903d5858100

10 | Oil pressure gauge indication is defective (oil pressure gauge needle does not move from the L position or less)
--- | ---
POSSIBLE CAUSE | • PCM malfunction • Instrument cluster malfunction • Oil pressure switch malfunction • Connector or pin malfunction • Short circuit in wiring harness between CAN-L, CAN-H and GND • Open circuit in CAN wiring harness (CAN-L, CAN-H) • CAN wiring harness (CAN-L, CAN-H) short each other

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Start the engine. • Does the oil pressure gauge needle indicate L position or more? | Yes | Troubleshooting completed.
No | Go to the next step.
2 | • Do the speedometer, the tachometer, and the water temperature gauge operate normally? | Yes | Go to the next step.
No | Go to Step 5.
3 | • Does the engine oil need replenishment? | Yes | Add the engine oil.
No | Go to the next step.
4 | • Start the instrument cluster input/output check mode. • Inspect the oil pressure gauge using the check code 28. • Is the oil pressure gauge normal? | Yes | Inspect the PCM, oil pressure switch, or connectors.
No | Replace the instrument cluster.
5 | • Start the engine. • Does the ABS warning light turn off? | Yes | Inspect the PCM or connectors.
No | Go to the next step.
6 | • Disconnect the negative battery cable. • Measure the resistance between the DLC-2 terminals F and E. • Is the resistance below 60 ohms? | Yes | Go to the next step.
No | Go to Step 8.
7 | • Disconnect the negative battery cable. • Inspect the DLC-2 terminals F and E for short to power supply or GND. • Is there any malfunction? | Yes | Inspect the wiring harness and CAN system-related module. Repair or replace the malfunctioning part.
No | Replace the instrument cluster.
8 | • Turn the ignition switch to LOCK position. • Inspect the instrument cluster connector terminals for poor connection (such as damaged/pulled-out pins, and corrosion). • Are the terminals normal? | Yes | Go to the next step.
| No | Repair or replace the terminal.
9 | • Disconnect the negative battery cable. • Measure the resistance between the instrument cluster connector terminals 1J and 1L. • Is the resistance 114—126 ohms? | Yes | Inspect the wiring harness and CAN system-related module. Repair or replace the malfunctioning part.
No | Replace the instrument cluster.