DIFFERENTIAL OIL REPLACEMENT

id031400800200

1. Park the vehicle on level ground.

2. Remove the oil-fill plug.

3. Remove the drain plug and drain the oil.

amxzzw00002369

4. Install the drain plug with a new washer and tighten.

  Tightening torque

  39.2—53.9 N·m {4.00—5.49 kgf·m, 29.0—39.7 ft·lbf}

5. Add the specified oil from the oil-fill plug hole until the oil level reaches the lower end of the plug hole.

amxzzw00001357

  Differential oil

  Grade: API service GL-5
  Viscosity: SAE 90
  Capacity (approx. quantity): 0.6—0.8 L {0.63— 0.85 US qt, 0.53—0.70 Imp qt}

6. Install the oil-fill plug with a new washer and tighten.

  Tightening torque

  39.2—53.9 N·m {4.00—5.49 kgf·m, 29.0—39.7 ft·lbf}