ACCELERATOR PEDAL REMOVAL/INSTALLATION [L8, LF]

id0113a3801400

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF])

3. Remove in the order indicated in the table.

amxzzw00000786

1 | Connector
2 | Accelerator pedal
3 | Accelerator pedal pad (If equipped)

4. Install in the reverse order of removal.