AIR INTAKE ACTUATOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1801400

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (3) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (4) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (5) Center panel unit (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

  (6) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (7) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (8) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (9) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (10) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (11) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (12) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (13) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (14) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (15) Bonnet release lever (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

  (16) Female bracket (See CONVERTIBLE TOP DISASSEMBLY/ASSEMBLY.)

  (17) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (18) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (19) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (20) Fuse box No.1

  (21) Dashboard (See DASHBOARD REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

L.H.D.

e5u740zw5001

R.H.D.

amxzzw00000692

1 | Air intake actuator connector
2 | Air intake actuator

5. Install in the reverse order of removal.