DTC P0500 [L8, LF]

id0102b1808400

DTC P0500 | VSS circuit problem
--- | ---
DETECTION CONDITION | • If an error in the wheel speed signal from the ABS HU/CM or DSC HU/CM is detected by CAN when the following conditions are met: ― Neutral switch and clutch pedal position switch: OFF (MT) ― Load: above 40% ― Engine speed: above 2,000 rpm ― Brake switch: OFF ― Shift lever position: P, N, R position (AT) Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA (Mode 2/Mode 12) is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • ABS HU/CM or DSC HU/CM malfunction ― Front ABS wheel-speed sensor malfunction ― Connector or terminals malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA (MODE 12) HAS BEEN RECORDED • Has the FREEZE FRAME DATA (Mode 12) been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA (Mode 12) on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY STORED DTC IN ABS HU/CM OR DSC HU/CM • Turn the ignition switch to the ON position (engine off). • Perform the Reading DTCs Procedure for ABS HU/CM or DSC HU/CM. (See ON-BOARD DIAGNOSIS [ABS].) (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See ON-BOARD DIAGNOSIS [ABS].) (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].)
No | Go to the next step.
4 | VERIFY DTC TROUBLESHOOTING COMPLETED • Turn the ignition switch to the ON position (engine off). • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Drive the vehicle under the following conditions for 18 s: ― Engine speed: above 2,000 rpm ― Gear: Gear is in other than NEUTRAL ― Load: above 40% • Perform the Pending Trouble Code Access Procedure. (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) • Is the PENDING CODE for this DTC present? | Yes | Replace PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
5 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [L8, LF].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF].)
No | DTC troubleshooting completed.