HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

id091800802000

Except Power Retractable Hardtop

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the partition board. (See PARTITION BOARD REMOVAL/INSTALLATION.)

4. Disconnect the high-mount brake light connector.

5. Press the tabs and remove the clips.

amxzzw00001098

6. Install in the reverse order of removal.

Power Retractable Hardtop

1. Fully open the deck panel.

2. Partially peel back the seal cover.

3. Disconnect the high-mount brake light connector.

4. Remove the wiring harness and connector of the high-mount brake light from the deck panel.

amxzzw00002145

5. Remove the nuts.

amxzzw00002028

6. Remove the high-mount brake light.

7. Install in the reverse order of removal.