INSTRUMENT CLUSTER OUTLINE

id092200100200

• The CAN system has been adopted for the control signals of the input/output communication circuit of the meters, gauges and warning and indicator lights. (See CONTROLLER AREA NETWORK (CAN) SYSTEM OUTLINE.)
• LEDs have been adopted for warning and indicator lights installed on the instrument cluster.
• A flat-type horn has been adopted.
• Due to the adoption of the power retractable hardtop, the power retractable hardtop warning alarm has been adopted.
• Malfunction warning light adopted. (With malfunction warning light)
• Active bonnet warning light and active bonnet warning alarm adopted. (With active bonnet system)