RADIATOR CONSTRUCTION [L8, LF]

id0112b4142000

• A cross-flow radiator with corrugated fins is used to improve cooling performance.
• The radiator tanks are made of plastic and the core is made of aluminum for weight reduction.
• Four rubber-insulated mounting brackets are utilized to decrease vibration.
• To improve both the cooling ability and allow the sporty design, the radiator is designed to tilt forward to reduce the height and to take in the air from the inlet installed under the bumper.
• The radiator has an ATF oil cooler in the right side radiator tank. (AT)

amxzzn00000566