CLUTCH RELEASE CYLINDER REMOVAL/INSTALLATION

id051000801300

  Caution
  • Fluid will damage painted surfaces. Be careful not to spill any fluid on painted surfaces. If fluid does get on painted surfaces, wipe it off immediately.

1. Remove the under guard. (LF engine MT models) (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].) (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Bleed the air from the system. (See CLUTCH FLUID REPLACEMENT.)

5. Inspect and adjust the clutch pedal. (See CLUTCH PEDAL ADJUSTMENT.)

amxzzw00000469

1 | Clutch pipe
2 | Clutch release cylinder