TRANSMISSION TECHNICAL DATA

id055000800200

Item | Specification
--- | ---
Pump housing bushing inner diameter | 38.113—38.138 mm {1.50051—1.50150 in}
Oil pump shaft bushing inner diameter | 21.501—21.527 mm {0.846496—0.847520 in}
Oil pump gear outer standard clearance | 0.10—0.17 mm {0.004—0.006 in}
Oil pump gear inner standard clearance | 0.07—0.15 mm {0.0028—0.0059 in}
Oil pump gear side standard clearance | 0.02—0.04 mm {0.0008—0.0015 in}
C1, C4 clutch return spring free length | Standard: 26.29 mm {1.04 in}
C2 clutch return spring free length | Standard: 20.02 mm {0.79 in}
C3 clutch return spring free length | Standard: 21.03 mm {0.83 in}
Input shaft component bushing inner diameter | 18.000—18.025 mm {0.7087—0.7096 in}
Clutch hub bushing inner diameter | Front side: 23.037—23.062 mm {0.90697—0.90795 in} Rear side: 23.037—23.062 mm {0.90697—0.90795 in}
Clutch hub component bushing inner diameter | Front side: 33.312—33.337 mm {1.31150—1.31248 in} Rear side: 33.312—33.337 mm {1.31150—1.31248 in}
B3 brake return spring free length | Standard: 15.72 mm {0.62 in}
B1 brake return spring free length | Standard: 17.05 mm {0.67 in}
Front planetary ring gear bushing inner diameter | 46.038—46.063 mm {1.81252—1.81350 in}
Front planetary gear component bushing inner diameter | 48.755—48.780 mm {1.91949—1.92047 in}
Rear planetary gear component bushing inner diameter | 18.000—18.025 mm {0.7087—0.7096 in}
B2 brake return spring free length | Standard: 22.66 mm {0.89 in}
B4 brake return spring free length | Standard: 13.84 mm {0.54 in}
Input shaft end play | 0.35—1.05 mm {0.014—0.041 in}
Distance A (between the end of the torque converter and the end of the converter housing) | MX-5 (ND): 21.4 mm {0.843 in} or more MX-5 (NC), RX-8 (SE): 26.2 mm {1.0 in}