AFTER REPAIR PROCEDURE [L8, LF]

id0102b1801100

1. Connect the M-MDS to the DLC‐2.

amxzzw00000605

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select the “Toolbox” tab.
    2. Select “Self Test”.
    3. Select “Modules”.
    4. Select “PCM”.
    5. Select “Retrieve CMDTCs”.

  • When using the PDS (Pocket PC)
    1. Select “Module Tests”.
    2. Select “PCM”.
    3. Select “Self Test”.
    4. Select “Retrieve CMDTCs”.

3. Verify the DTC according to the directions on the M-MDS screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Verify that no DTCs are displayed.