NEUTRAL SWITCH REMOVAL/INSTALLATION [P66M-D]

id051111247100

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

4. Remove the neutral switch.

amxzzw00000512

5. Install the neutral switch and a new packing to the transmission case.

  Tightening torque

  23.6—35.3 N·m
  {2.5—3.5 kgf·m, 18—26 ft·lbf}

6. Install the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)