DOUBLE LOCKING SYSTEM OUTLINE

id091400593500

• The double locking system disables unlock operation of the lock knob when all the doors and the trunk lid are closed and locked two times consecutively. The operation conditions of the double locking system are as follows:

  ― The doors and the trunk lid are locked twice within approx. 3 s using the LOCK button on the transmitter.
  ― The doors and the trunk lid are locked twice within approx. 3 s using the key.