ON-BOARD DIAGNOSTIC SYSTEM ACTIVE COMMAND MODES FUNCTION [DYNAMIC STABILITY CONTROL (DSC)]

id0402b2175300

• The active command modes function is used for optionally selecting active command modes items of input/output parts preset in the DSC HU/CM, and to operate them regardless of CM control.
• To protect the hydraulic unit interior, operate output related parts for only 10 s or less when using the active command modes function.

Active Command Modes Table

Command name | Output part name | Operation | Operation condition
--- | --- | --- | ---
LATACCEL | Combined sensor (lateral acceleration) initialization | FALSE/TRUE | Ignition switch at ON
LF_INLET | LF inlet solenoid valve | Off/On
LF_OUTLET | LF outlet solenoid valve
LR_INLET | LR inlet solenoid valve
LR_OUTLET | LR outlet solenoid valve
PMP_MOTOR | Pump motor
RF_INLET | RF inlet solenoid valve
RF_OUTLET | RF outlet solenoid valve
RR_INLET | RR inlet solenoid valve
RR_OUTLET | RR outlet solenoid valve
SAS_CAL | Steering angle sensor initialization | FALSE/TRUE
STAB_IND | DSC indicator light | Off/On
TRAC_OFF | DSC OFF switch
V_STB_L | LH stability control solenoid valve
V_STB_R | RH stability control solenoid valve
V_TRC_L | LH traction control solenoid valve
V_TRC_R | RH traction control solenoid valve
YAWRATE | Combined sensor (yaw rate) initialization