DECORATION PANEL REMOVAL/INSTALLATION

id091700788200

Driver’s Side

1. Pull the decoration panel outward and detach clips A.

amxzzw00001410

2. Remove the decoration panel.

3. Install in the reverse order of removal.

Passenger’s Side

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Center panel unit (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

4. Remove the three screws.

e5u917zw5019

5. Pull the decoration panel outward and detach clips A and B.

6. Remove the decoration panel.

7. Install in the reverse order of removal.