CONVERTIBLE TOP ADJUSTMENT

id091600807900

1. Remove the spring.

e5u916zw8000

2. Remove the snap ring. (See Snap Ring Removal Note.) (See Snap Ring Installation Note.)

3. Remove the pin.

4. Remove the screws.

5. Remove the cover.

6. Adjust the clearance of part A by rotating the adjustment nut.

  Note
  • Turn the adjustment nut to the right to narrow the part A clearance, left to widen it.

e5u916zw8008

  Clearance

  A: 4—8 mm {0.16—0.31 in}

7. Install in the reverse order of removal.

Snap Ring Removal Note

  Caution
  • Remove the snap ring such that the dimension is maintained as indicated in the figure.

  e5u916zw8002

  • Because the snap ring is to be reused, remove it carefully so that the ring is not expanded.

1. Insert a tape-wrapped flathead screwdriver between the cover and snap ring, and remove the snap ring by prying along the perimeter so as not to damage the snap ring.

e5u916zw8001

Snap Ring Installation Note

1. Insert the snap ring to the pin while slightly expanding the snap ring end using snap ring pliers.

e5u916zw8003

2. After securing the snap ring, verify that there is no excessive play between the snap ring and pin.