MASTER CYLINDER CONSTRUCTION

id041100100700

• A plunger-type master cylinder with a 22.2 mm {0.87 in} bore has been adopted, improving durability.

  Note
  • Plunger type: A system where the cups are fixed on the cylinder, and the piston slides through the inner perimeter of the cups.

• For vehicles with DSC, the master cylinder outlet pipe diameter has been increased, improving response during DSC operation.
• Except for the reservoir, the master cylinder cannot be disassembled. Therefore, if there is any malfunction in the interior of the master cylinder, replace the cylinder component without disassembling.

amxzzn00000172