WIPER AND WASHER SWITCH REMOVAL/INSTALLATION

id091900800200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

4. Disconnect the wiper and washer switch connector.

amxzzw00000731

5. Remove the screws, then remove the wiper and washer switch.

6. Install in the reverse order of removal.