ON-BOARD DIAGNOSTIC SYSTEM MALFUNCTION DISPLAY FUNCTION [L8, LF]

id0102b1142000

Outline

• Illuminates the malfunction indicator lamp to notify the driver of a malfunction occurring in the engine control system.
• The malfunction indicator lamp is in the instrument cluster.

amxzzn00000228

Function

• The malfunction indicator lamp illuminates when a malfunction occurs in the engine control system, and it illuminates at the same time a DTC is recorded in the PCM.
• The illumination/non-illumination conditions of the malfunction indicator lamp are determined by the number of drive cycles. (See ON-BOARD DIAGNOSTIC SYSTEM TEST MODE [L8, LF].)