WIPER MOTOR DISASSEMBLY/ASSEMBLY

id091900804600

1. Disassemble in the order indicated in the table.

e5u919zw5016

1 | Bolt
2 | Wiper motor (See Wiper Motor Assembly Note.)
3 | Wiper link No.1 (See Ball Joint Assembly Note.)
4 | Wiper link No.2 (See Ball Joint Assembly Note.)
5 | Main link (See Ball Joint Assembly Note.)

2. Assemble in the reverse order of disassembly.

Ball Joint Assembly Note

1. Use a clean rag to protect the link, and squeeze using pliers.

amxzzw00002296

Wiper Motor Assembly Note

1. Connect the wiper motor to the vehicle wiring harness connector, operate the wipers, and then stop them at the auto-stop position.

2. Adjust the motor crank, wiper link No.1 and wiper link No.2 so that they are parallel as shown in the figure.

e5u919zw5018

3. Assemble the wiper motor.