CLUTCH MASTER CYLINDER REMOVAL/INSTALLATION

id051000801400

  Caution
  • Fluid will damage painted surfaces. Be careful not to spill any fluid on painted surfaces. If it is spilled, wipe it off immediately.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Bleed the air from the system. (See CLUTCH FLUID REPLACEMENT.)

4. Inspect and adjust the clutch pedal. (See CLUTCH PEDAL ADJUSTMENT.)

amxzzw00000470

1 | Hose clip
2 | Clutch pipe
3 | Nut
4 | Clutch master cylinder
5 | Packing