ACCELERATOR PEDAL POSITION (APP) SENSOR INSPECTION [L8, LF]

id0140i7803200

1. Connect the M-MDS to the DLC‐2.

amxzzw00000042

2. Turn the ignition switch to the ON position.

3. Verify that the APP sensor output voltage (PID: APP1, APP2) increases according to the increase in the accelerator opening angle when the accelerator opening angle is gradually increased.

• If verified, go to the next step.
• If not as verified, replace the accelerator pedal. (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [L8, LF].)

4. Verify that the APP sensor output voltage (PID: APP1, APP2) is within the specification when the accelerator pedal is depressed and not depressed.

• If not as specified, replace the accelerator pedal. (See ACCELERATOR PEDAL REMOVAL/INSTALLATION [L8, LF].)