VENTILATOR GRILLE REMOVAL/INSTALLATION

id091700454100

Driver’s Side

1. Remove the decoration panel. (driver’s side) (See DECORATION PANEL REMOVAL/INSTALLATION.)

2. Remove the screws.

e5u917zw5011

3. Remove the ventilator grille.

4. Install in the reverse order of removal.

Passenger’s Side

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Center panel unit (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (5) Decoration panel (passenger’s side) (See DECORATION PANEL REMOVAL/INSTALLATION.)

4. Remove the screws.

amxzzw00001399

5. Remove the ventilator grille.

6. Install in the reverse order of removal.

Center

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Center panel unit (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

  (4) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (5) Decoration panel (passenger’s side) (See DECORATION PANEL REMOVAL/INSTALLATION.)

4. Remove the screws.

amxzzw00001400

5. Remove the ventilator grille.

6. Install in the reverse order of removal.