COIL ANTENNA REMOVAL/INSTALLATION

id091400804900

  Note
  • Do not remove the coil antenna unless you are replacing it.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Disconnect the coil antenna connector.

amxzzw00000580

4. Detach the steering lock tabs from the holes on the coil antenna.

5. Install in the reverse order of removal.