ON-BOARD DIAGNOSTIC SYSTEM OUTLINE [ACTIVE BONNET]

id0802f1003500

• The active bonnet has an on-board diagnostic function to facilitate system diagnosis.
• The on-board diagnostic function has the following functions:

  ― Malfunction detection function: Detects overall malfunctions in the active bonnet-related parts.
  ― Fail-safe function: Stops the active bonnet actuator from deploying mistakenly if the active bonnet is malfunctioning.
  ― Memory function: Stores detected malfunctions.
  ― Display function: Notification of system malfunction by displaying DTCs.
  ― PID/data monitor function: Reads specific input/output signals.

• Using the Mazda Modular Diagnostic System (M-MDS), DTCs can be read out and deleted, and PID/data monitoring can be performed.