REAR COMBINATION LIGHT REMOVAL/INSTALLATION

id091800465500

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

4. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

amxzzw00001055

1 | Nut
2 | Connector
3 | Rear combination light
4 | Socket
5 | Brake light/taillight bulb
6 | Rear turn light bulb
7 | Back-up light bulb (passenger-side only) Rear fog light bulb (driver-side only) (with rear fog light)

6. Install in the reverse order of removal.