IGNITION KEY ILLUMINATION OPERATION

id091800101400

Illumination Condition

• The ignition key illumination glows under all of the following conditions.

  ― Driver-side door is open. (Driver-side door switch is on.)
  ― Ignition switch is at the LOCK or ACC position. (IG1 off)

Cancel Condition

• The ignition key illumination goes out under any of the following conditions.

  ― Approx. 30 s after all doors are closed. (Approx. 30 s after all door switches are off.)
  ― Ignition switch is at the ON position. (IG1 on)
  ― Approx. 5 min after ignition key illumination begins.