FUEL-FILLER LID OPENER LEVER AND CABLE REMOVAL/INSTALLATION

id091400808800

Fuel-filler Lid Opener Lever

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Seats (See SEAT REMOVAL/INSTALLATION.)

  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (3) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (4) Scuff plate (SCUFF PLATE REMOVAL/INSTALLATION.)

  (5) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (6) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (7) Seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (8) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (9) Seat back bar lower garnish (See SEAT BACK BAR LOWER GARNISH REMOVAL/INSTALLATION.)

3. Remove the nut.

amxzzw00000563

4. Remove the fuel-filler lid opener lever.

5. Install in the reverse order of removal.

6. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)

Fuel-filler Lid Opener Cable

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Seats. (See SEAT REMOVAL/INSTALLATION.)

  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (3) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (4) Scuff plate (SCUFF PLATE REMOVAL/INSTALLATION.)

  (5) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (6) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (7) Seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (8) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (9) Seat back bar lower garnish (See SEAT BACK BAR LOWER GARNISH REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (12) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (13) Fuel-filler lid opener (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

3. Remove the fuel-filler lid opener cable.

amxzzw00000564

4. Install in the reverse order of removal.

5. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)