REAR FENDER PANEL REMOVAL [PANEL REPLACEMENT]

id098008744900

1. Drill the 65 locations (vehicle with convertible top)/64 locations (vehicle with power retractable hardtop) indicated by (A), 17 locations indicated by (B), and 2 locations (vehicle with convertible top only) indicated by (C), then remove the rear fender panel.

  Note
  • Drilling of the 17 location indicated by (B) is not necessary when removing the rear fender panel and the side sill reinforcement (rear) at the same time.

  amxuub00000002

2. Remove the rear fender panel.

  Note
  • For weld the 2 location (C), partially bend back the rear deck panel before drilling.

3. Remove the spot weld sealer using a disc grinder.

Convertible Top

amxuub00000003

Power Retractable Hardtop

amxuub00000004