ANTENNA FEEDER NO.2 REMOVAL/INSTALLATION

id092000812300

Except Power Retractable Hardtop

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Seat (RH) (See SEAT REMOVAL/INSTALLATION.)

  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (3) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (4) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (5) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (6) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (7) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (8) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (9) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (10) Seat belt set plate (See SEAT BELT REMOVAL/INSTALLATION.)

  (11) Seat back crossmember assembly (See SEAT BACK CROSSMEMBER ASSEMBLY REMOVAL/INSTALLATION.)

  (12) Rear side trim (See REAR SIDE TRIM REMOVAL/INSTALLATION.)

  (13) Rear package trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

  (14) Side shelf (RH) (See SIDE SHELF REMOVAL/INSTALLATION.)

  (15) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (16) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (17) Trunk side trim (RH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

4. Disconnect the antenna feeder No.1.

amxzzw00001690

5. Remove the clip A.

6. Partially peel back the floor covering.

7. Detach clips B.

amxzzw00001691

8. Detach clips C.

amxzzw00001692

9. Disconnect the wiring harness from the clip D.

amxzzw00001693

10. Disconnect the connector.

11. Detach clips D and E.

12. Remove the antenna feeder No.2.

13. Install in the reverse order of removal.

Power Retractable Hardtop

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Seat (RH) (See SEAT REMOVAL/INSTALLATION.)

  (2) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (3) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (4) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (5) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (6) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (7) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (8) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (9) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (10) Rear side trim (See REAR SIDE TRIM REMOVAL/INSTALLATION.)

  (11) Side shelf (RH) (See SIDE SHELF REMOVAL/INSTALLATION.)

  (12) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (13) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (14) Trunk side trim (RH) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

4. Disconnect the antenna feeder No.1.

amxzzw00001694

5. Remove the clip A.

6. Partially peel back the floor covering.

7. Detach clips B.

amxzzw00001695

8. Detach clips C.

amxzzw00001696

9. Disconnect the wiring harness from the clip D.

amxzzw00001697

10. Disconnect the connector.

11. Detach clips D and E.

12. Remove the antenna feeder No.2.

13. Install in the reverse order of removal.