CENTER SPEAKER REMOVAL/INSTALLATION

id092000806000

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove in the order indicated in the table.

amxzzw00002307

1 | Center speaker cover (See Center Speaker Cover Removal Note.)
2 | Screw
3 | Center speaker
4 | Connector

4. Install in the reverse order of removal.

Center Speaker Cover Removal Note

1. Insert a tape-wrapped fastener remover into the service hole.

e5u920zw5012

2. Pry with the tape-wrapped fastener remover in the direction shown by the arrow to remove the center speaker cover.