VARIABLE TUMBLE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF]

id0113a3810100

1. Remove the plug hole plate. (See PLUG HOLE PLATE REMOVAL/INSTALLATION [L8, LF].)

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

amxzzw00000813

1 | Connector
2 | Vacuum hose
3 | Variable tumble solenoid valve