GENERATOR CONTROL OUTLINE [L8, LF]

id0140i7172300

• Idling stability and the corresponding load performance have been improved by optimum control of generator voltage according to engine operation and electrical load conditions.
• The PCM determines the engine operation and electrical load conditions based on the input signals from input devices shown in the figure below and controls the excitation time of the generator field coils.