SIDE TURN LIGHT REMOVAL/INSTALLATION

id091800811500

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Move the side turn light in the direction of the arrow (1) and detach the tab.

amxzzw00001020

4. Pull area A of the side turn light in the direction of the arrow (2) and remove the front side turn light.

5. Disconnect the side turn light connector.

amxzzw00001021

6. Remove the side turn light

7. Remove the socket.

8. Remove the side turn light bulb.

9. Install in the reverse order of removal.