AUXILIARY JACK INSPECTION

id092000812600

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (3) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (4) Auxiliary jack (See AUXILIARY JACK REMOVAL/INSTALLATION.)

4. Connect a commercially-available nonresistant plug to the auxiliary jack.

amxzzw00001686

5. Verify that the continuity between the auxiliary jack terminals is as indicated in the table.

amxzzw00001687

  • If not as indicated in the table, replace the auxiliary jack.