REFRIGERANT LINE CONSTRUCTION

id071100806500

• Aluminum alloy has been adopted for the pipes of the refrigerant lines and rubber (flexible hoses) has been adopted for the hoses.
• A high-pressure charging valve is installed on cooler pipe No.2, and a low-pressure charging valve is installed on the cooler pipe No.3 (L.H.D.), cooler hose (LO) (R.H.D.)

L.H.D.

amxzzn00000333

R.H.D.

amxzzn00000334