DRIVELINE/AXLE SPECIFICATIONS

id030000100200

Item | Specification
--- | ---
Transmission type | L8/5MT | LF/5MT | LF/6MT | LF/6EAT
Front axle
Bearing type | Angular ball bearing
Rear axle
Bearing type | Angular ball bearing
Rear drive shaft
Joint type | Wheel side | Bell joint
Differential side | Tripod joint
Shaft diameter | (mm {in}) | 36.0 {1.42} (Maximum diameter) 26.6 {1.05} (Minimum diameter)
Rear differential
Reduction gear type | Hypoid gear
Differential gear type | Straight bevel gear
Ring gear size | (inch) | 7.35
Reduction ratio | 3.909 | 4.100 | 3.727 | 4.100
Number of gear teeth | Drive pinion | 11 | 10 | 11 | 10
Ring gear | 43 | 41
Differential oil | Type | Grade | API service GL-5
Viscosity | SAE 90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 0.6—0.8 {0.63—0.85, 0.53—0.70}
Propeller shaft
Length |  | (mm {in}) | L | 736 {29.0} | 780 {30.7}
Diameter |  | (mm {in}) | D | 65 {2.6}